**Product 1 – Paper Surface Board (Both laminated and non-laminated)**

About Rubberised Board Rubberised board is well known for its well tensile strength , highly flexible nature and very high bursting factor . The material is very well accepted in the aluminium and steel industry both inland and abroad. The raw material used in manufacturing of rubberised board is of world class quality and the product is eco-friendly.

The percentage of components is mentioned below:

**ITEM NAME AND PERCENTAGE**

1) VIRGIN CRAFT CUTTING - 30%

2) VIRGIN WHITE PAPER CUTTING - 50%

3) CHEMICALS - 10%

4) BAMBOO - 5%

5) RESIN AND ADHESIVE - 5%

The process of its manufacturing is illustrated through a flow chart on the next page.

**Conclusion**

It feels pride to develop such a eco-friendly material which is the sole solution for aluminium and steel industry. The world-wide acclaim for it is also due to its cost effectiveness as compared to other materials in its category.